This specification section is provided in CSI-format, and intended to be included in the Project Manual for a construction project.  Delete models and options not required for your project, and modify to your project requirements.


SECTION 102814

ADULT CHANGING STATIONS

PART 1: GENERAL

SECTION INCLUDES

Adult Changing Stations, Adjustable Height:
Adjustable-Height Adult-Changing Station (Koala Model KB2600)
 
RELATED REQUIREMENTS

Section 061000 - Rough carpentry, blocking in walls.

Section 092100 - Plaster and gypsum board assemblies, blocking in walls.

Section 093000 - Tiling, coordination with tile layout and installation.

Section 260000 – Electrical service installation.

SUBMITTALS

Product Data:  Submit manufacturer's data sheets for each product specified, including the following.
0. Installation instructions and recommendations, including templates and rough-in measurements.
0. Storage and handling requirements and recommendations.
0. Cleaning and maintenance instructions.

QUALITY ASSURANCE

Manufacturer:  Provide products manufactured by a company with a minimum of 5 years successful experience manufacturing similar products.

Single Source Requirements:  To the greatest extent possible provide products from a single manufacturer.

Accessibility Requirements:  Comply with requirements applicable in the jurisdiction of the project, including but not limited to ADA, ICC A117.1 International Building Code (IBC), and state building code requirements as applicable.

Manufacturing Location:  United Kingdom

DELIVERY, STORAGE, AND HANDLING

Deliver, store and handle materials and products in strict compliance with manufacturer's instructions and recommendations.  Protect from damage.

WARRANTY 

Manufacturer’s Warranties:  Submit manufacturer’s standard 3 year warranty for materials and workmanship.


PART 2: PRODUCTS

1. 
MANUFACTURER

Basis of Design Products: Based on the quality and performance requirements of the project, specifications are based solely on the products of Koala Kare Products, a Division of Bobrick, www.koalabear.com. 

Substitutions:  The Architect will consider products of comparable manufacturers as a substitution, pending the contractor's submission of adequate documentation of the substitution in accordance with procedures in Division 1 of the Project Manual.  Documentation shall include a list of five similar projects of equivalent size where products have been installed for a minimum of two years.

ADULT CHANGING STATIONS, HEIGHT-ADJUSTABLE

Surface-Mounted Adjustable Height Changing Station :  
Basis of Design:  Model KB2600 as manufactured by Koala Kare Products, a Division of Bobrick.
[bookmark: _Hlk210030122]Powered-Height Adjustability: Changing surface shall electronically adjust from 14” (350mm) to 37” (950 mm) from floor. 
Weight Capacity: Tested to support up to 440 lbs. (200 kg.) static load.
Unit shall be UL and ULc listed.
Station shall have UL 962 & C22.2 No. 68 certification. 
[bookmark: _Hlk210030318]Changing Surface shall be a minimum 71” (1800 mm) wide, and 31.5” (800mm) deep 
Changing Surface shall be non-rip, high tension vinyl.  
Back-Up Battery: Unit shall have a fail-safe backup battery that allows for continuous operation in the event of a power interruption. 
Class 1 electrical system to protect against electrical shock. 
Integrated handheld control to automatically adjust height.
Unit shall have an integrated guard that allows for single handed operation and a lift/drop locking mechanism that allows easy rotation to stow. 
Unit shall be IPX4 water resistant. 
Changing surface durable, non-rip, high tension, vinyl stretcher that is easy to clean. 
All moving parts shall be concealed or guarded in such a way to protect against pinch points or entrapment. 
Unit shall have Full IEC 60601-1 certified including US, EU and Canadian differences. 
Frame shall be constructed of powder coated tubular steel. 

PART 3: EXECUTION

2. 
INSTALLATION

Install products in strict compliance with manufacturer’s written instructions and recommendations, including the following:
0. Verify wall blocking has been installed properly.
0. Verify required electrical services have been installed properly. 
0. Verify wall location does not interfere with door swings or use of fixtures.
0. Use fasteners and anchors suitable for wall substrate and project conditions.
0. Install units at location and height indicated on the drawings.
0. Install units level, plumb, and in proper relationship with adjacent construction.
0. Adjust for proper operation.

PROTECTION

Protect installed products until completion of project.

Touch-up, repair or replace damaged products before substantial completion.
	
	END OF SECTION



